**20mm PANEL (INTERNAL USE)**

To produce 1,000m2 of PAL Pre-insulated Ducting System, the following is a list of material and accessories for a standard construction requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **CODE** | **DESCRIPTION** | **UOM** | **APPROX. QTY.** |
| 20P80 | Panel 4000 x 1200mm | m2 | 1,100 |
| 20AC10 | Aluminum Invisible Profile | mtr | 760 |
| 20AC11 | H Bayonet in Polymer | mtr | 400 |
| 20AC12 | Corner Cover in Polymer | pc | 900 |
| 20AC13 | Corner Plate for Invisible Profile | pc | 1,200 |
| 20AC14 | Aluminum U Profile | mtr | 80 |
| 20AC15 | Aluminum Chair Profile | mtr | 80 |
| 20AC16 | Aluminum F Profile | mtr | 80 |
| M23 | PAL Adhesive | kg | 90 |
| 20M24 | Aluminum Tape | roll | 150 |
| M25 | PAL Sealant | tube | 90 |