**30mm PANEL (EXTERNAL USE)**

To produce 1,000m2 of PAL Pre-insulated Ducting System, the following is a list of material and accessories for a standard construction requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **CODE** | **DESCRIPTION** | **UOM** | **APPROX. QTY.** |
| 30P200 | Panel 4000 x 1200mm | m2 | 1,100 |
| 30AC10 | Aluminum Joint Profile | mt | 760 |
| 30AC11 | Aluminum Channel | mt | 400 |
| 30AC12 | Steel Corner | pc | 1,500 |
| M30 | Gasket | pc | 400 |
| 30AC14 | Aluminum U Profile | mt | 80 |
| 30AC15 | Aluminum Chair Profile | mt | 80 |
| 30AC16 | Aluminum F Profile | mt | 80 |
| M23 | PAL Adhesive | kg | 90 |
| 30M24 | Aluminum Tape | roll | 150 |
| M25 | PAL Sealant | tube | 90 |
| M26 | Thermal Insulation Tape | mt | 300 |
| AC18 | Reinforcement Bar in Aluminum | mt | 120 |
| AC19 | Reinforcement Disc | pc | 200 |